SIMATIC S7 MatLab Toolbox

### - a -

- Address : IPDeviceEndPoint, PlcValue

### - b -

- BitNumber : PlcAddress
- BreakDetectionTimeout : PlcDeviceConnection
- ByteNumber : PlcAddress

### - c -

- ChannelType : SimaticDevice
- Connection : PlcDevice
- ConnectTimeout : PlcDeviceConnection
- Counter : PlcOperand

### - d -

- DefaultRack : IPDeviceEndPoint
- DefaultSlot : IPDeviceEndPoint
- DefaultTimeout : PlcDeviceConnection

### - f -

- Flag : PlcOperand

### - i -

- Input : PlcOperand
- IsCustomRack : IPDeviceEndPoint
- IsCustomSlot : IPDeviceEndPoint

### - l -

- Length : PlcArray

### - m -

- ManagedInstance : PlcDevice, PlcDeviceConnection, PlcOperand, PlcValue
- MaxRack : IPDeviceEndPoint
- MaxSlot : IPDeviceEndPoint
- MinRack : IPDeviceEndPoint
- MinSlot : IPDeviceEndPoint

### - n -

- Number : PlcOperand

### - o -

- OperandNumber : PlcAddress
- OperandType : PlcAddress
- Output : PlcOperand

### - p -

- PeripheryInput : PlcOperand
- PeripheryOutput : PlcOperand

### - r -

- Rack : IPDeviceEndPoint
- RawType : PlcAddress
- ReceiveTimeout : PlcDeviceConnection

### - s -

- Slot : IPDeviceEndPoint
- State : PlcDeviceConnection

### - t -

- Timer : PlcOperand
- TransmitTimeout : PlcDeviceConnection
- Type : PlcOperand, SimaticDevice

### - u -

- UseBreakDetection : PlcDeviceConnection

### - v -

- Value : PlcAddress, PlcBoolean, PlcBooleanArray, PlcByte, PlcByteArray, PlcChar, PlcCharArray, PlcDate, PlcDateTime, PlcDouble, PlcDoubleArray, PlcInt16, PlcInt16Array, PlcInt32, PlcInt32Array, PlcReal, PlcRealArray, PlcS5Time, PlcString, PlcTime, PlcTimeOfDay, PlcUInt16, PlcUInt16Array, PlcUInt32, PlcUInt32Array, PlcValue