********** CONNECT-CONTROL **********
*************************************

1.) The device is a CONNECT-CONTROL
===================================
Please call up the menu item "Firmware-Update" in the web interface of the CONNECT-CONTROL and 
search for the path of the extracted file "tlt_custom_pkg_connect-rut9xx_Y.YY.01.ipk" in the 
opened dialog and accept the file. ("Y" is a placeholder for the respective version) 
The selected file is loaded and then burned in the flash-memory. After restarting the device, 
it can be addressed with the new firmware-version. 

2.) The device is a router from Teltonika that is to be used as a CONNECT-CONTROL
=================================================================================
If the router used does not have the basic-firmware-version "06.07.7" or is more recent, please 
carry out a firmware-update via the web interface with the file "RUT9XX_R_00.06.07.7_WEBUI.bin".
!!! Without this basic firmware version, the CONNECT software extension cannot be installed 
and used !!!
The firmware-update-process is described in your router-manual. 
Start up the device with the basic-firmware-version "06.07.1" and load under 
"System" => "Package-Manager" => "Update" the firmware file "tlt_custom_pkg_connect-rut9xx_Y.YY.01.ipk"
into the device. ("Y" is a placeholder for the respective version) 
After restarting the device, it can be addressed with the new firmware version.




