How to install the Demo for S7-VISU
===================================

Steps for the S7-PLC:

1.Locate one the STEP7 projects in the examples folder and load it into your STEP7
2.If necessary replace the S7-PLC in the project to your specific one in use 
3.Load the project into your S7-PLC 
4.Connect the netSCADA device to the PLC physically over the MPI/PROFIBUS interface
5.Switch the PLC to RUN mode


Steps for the S7-VISU:

1.Locate the "atvise Demo.xml" file in the example folder
2.In atvise Builder use menu item "builder/import(absolute) from XML..." to import "ativse Demo.xml"
3.Use menu item "builder/disconnect from server" to stop the background server
4.Use menu item "builder/connec to server" to restart the server again
5.The "Atvise Demo" server will get present in the Servers Tree List
6.Double click the "atvise Demo" server and change the given IP address to the IP address of your device and press OK.
7.Use menu item "Guided Actions/Distribute to Webserver/Atvise Demo" to download visualization into your device
8.Use menu item "Guided Actions/Open Web Browser for Server/Atvise Demo" to open you standard web browser to watch the Demo Sites.



